Anexa nr.3

la Cerinţele de calitate

pentru orez şi crupe de orez

**Ponderea boabelor defecte**

**în diferite tipuri de orez**

(în %)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Boabe defecte** | **Orez decorticat** | **Orez albit** | **Orez decorticat prefiert** | **Orez albit prefiert** |
| Boabe atacate de căldură | 4,0 | 3,0 | 8,0 | 6,0 |
| Boabe deteriorate | 4,0 | 3,0 | 4,0 | 3,0 |
| Boabe nedezvoltate | 12,0 | 2,0 | 12,0 | 2,0 |
| Boabe albicioase | 11,0 | 11,0 | nu se admite | nu se admite |
| Boabe roşii | 12,0 | 4,0 | 12,0 | 4,0 |
| Boabe striate cu roşu | nu se admite | 8,0 | nu se admite | 8,0 |
| Boabe pătate | nu se admite | nu se admite | 4,0 | 2,0 |